**Zoning on Brocade Switch**

**Overview**

|  |  |  |  |
| --- | --- | --- | --- |
| **Trigger:** | Zoning On Brocade Switch | | |
| **Special Permissions:** | SAN Switch Admin | **Responsible Team:** | Storage Team |
| **Config. Item:** | Brocade Switches | **KB Reference:** | KB# |

**Instructions**

|  |  |
| --- | --- |
| **Step #** | **Information** |
| 1. | Brocade switch configuration needs to be backed up before any modifications on the fabrics Using “configupload” command. |
| 2. | **Alias Creation:-** alicreate “Name”,”portname1/WWPN" |
| 3. | **Zone creation & adding to active zoneset:-** zonecreate “Zone Name”, “Initiator alias1; Target alias2″ |
| 4. | Add the newly created zones to the active zoneset with the following syntax:- cfgadd “ConfigName”, “Zonename1;Zonename2,etc″ |